Firmware Details
================
1chipmsx_br_layout\bios_msx2plus_backslash      <=  this fw is for 1chipMSX with Brazilian keyboard / MSX2+ logo
                  \bios_msx3_backslash          <=                 1chipMSX with Brazilian keyboard / MSX3  logo
1chipmsx_es_layout\bios_msx2plus_backslash      <=  this fw is for 1chipMSX with Spanish   keyboard / MSX2+ logo
                  \bios_msx3_backslash          <=                 1chipMSX with Spanish   keyboard / MSX3  logo
1chipmsx_fr_layout\bios_msx2plus_backslash      <=  this fw is for 1chipMSX with French    keyboard / MSX2+ logo
                  \bios_msx3_backslash          <=                 1chipMSX with French    keyboard / MSX3  logo
1chipmsx_jp_layout\bios_msx2plus_yen            <=  this fw is for 1chipMSX with Japanese  keyboard / MSX2+ logo
                  \bios_msx3_yen                <=                 1chipMSX with Japanese  keyboard / MSX3  logo
1chipmsx_uk_layout\bios_msx2plus_backslash      <=  this fw is for 1chipMSX with English   keyboard / MSX2+ logo
                  \bios_msx3_backslash          <=                 1chipMSX with English   keyboard / MSX3  logo

zemmixneo_br_layout\bios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean     with Brazilian keyboard
                   \bios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian  with Brazilian keyboard
                   \bios_sx1_backslash          <=                 8bits4ever SX-1 Board with Brazilian keyboard
zemmixneo_es_layout\bios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean     with Spanish   keyboard
                   \bios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian  with Spanish   keyboard
                   \bios_sx1_backslash          <=                 8bits4ever SX-1 Board with Spanish   keyboard
zemmixneo_fr_layout\bios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean     with French    keyboard
                   \bios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian  with French    keyboard
                   \bios_sx1_backslash          <=                 8bits4ever SX-1 Board with French    keyboard
zemmixneo_jp_layout\bios_zemmixneo_yen          <=  this fw is for Zemmix Neo Korean     with Japanese  keyboard
                   \bios_zemmixneobr_yen        <=                 Zemmix Neo Brazilian  with Japanese  keyboard
                   \bios_sx1_yen                <=                 8bits4ever SX-1 Board with Japanese  keyboard
zemmixneo_uk_layout\bios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean     with English   keyboard
                   \bios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian  with English   keyboard
                   \bios_sx1_backslash          <=                 8bits4ever SX-1 Board with English   keyboard


DIP-SW and Special Keys
=======================
GRAPH              <=  [ALT]
KANA/CODE          <=  [F7]
SELECT             <=  [F8]
CPU Clock          <=  [F12] or [DIP-SW1]
Video Output       <=  [(SHIFT+)PRNSCR] or [DIP-SW2/3]
Audio Mixer & CMT  <=  [(SHIFT+)PGUP/PGDOWN/F9/F10/F11] & [SCRLCK]
Cartridge Slot-1   <=  [SHIFT+F12] or [DIP-SW4]
Cartridge Slot-2   <=  [SHIFT+SCRLCK] or [DIP-SW5/6]
System Reset       <=  [HARD RESET KEY] Fast or Long-Click (normal or full reboot)
Internal Mapper    <=  [DIP-SW7] only
Internal MegaSD    <=  [DIP-SW8] only

______________
KdL 2019.05.20
