OCM-PLD Pack v3.9.1
===================

Author:  KdL
Update:  2022.09.24

This package includes a set of custom firmware to update the following machines.
1st Gen  =>  1chipMSX, Zemmix Neo (KR), Zemmix Neo BR, SX-1 (regular) and SX-1 Mini/Mini+.
2nd Gen  =>  SM-X (regular) and SX-2. [!] SM-X Mini is no longer supported by me.

Any content of this package is NOT intended for a commercial purpose and is for personal use only.
The author disclaims any liability for the misuse of the contents of this package.

All firmware are self-made and not provided by the respective manufacturers.
However, manufacturers are allowed to use these firmware as long as no surcharge is applied.
The common base firmware is that of the first generation, which originated with 1chipMSX.
Second generation machines have additional functions as they are more capacious.

The MSX++ logo was officially granted to the OCM-PLD firmware by 西 和彦 [Mr. Kazuhiko Nishi] on 2022/Jul/21st.

Here is how to recognize an MSX++ system and how it is classified:
- the 1chipMSX machine upgraded with OCM-PLD is for all intents and purposes an MSX++ computer;
- while homebrew machines that receive the same type of upgrade are considered MSX++ compatible;
- individual components do not identify MSX++, so all unofficial firmware derived from OCM-PLD
  (those not maintained by me) can be considered MSX++ compatibles as long as they correcly support
  the switched I/O ports extension with ID 0xD4 (212=OCM ID, now MSX++ ID).

For more details, refer to the 'history.txt' and the other texts included in the folders of this package.


______
Enjoy!
