Firmware list divided into interchangeable groups
=================================================
                                                                                                                                    { GROUP 1 }
 1chipmsx_br_layout\single_epbios_msxplusplus_backslash  <=  this fw is for 1chipMSX                with Brazilian keyboard / MSX++ official logo
                   \single_epbios_msx2plus_backslash     <=                 1chipMSX                with Brazilian keyboard / MSX2+ logo
 1chipmsx_es_layout\single_epbios_msxplusplus_backslash  <=  this fw is for 1chipMSX                with Spanish   keyboard / MSX++ official logo
                   \single_epbios_msx2plus_backslash     <=                 1chipMSX                with Spanish   keyboard / MSX2+ logo
 1chipmsx_fr_layout\single_epbios_msxplusplus_backslash  <=  this fw is for 1chipMSX                with French    keyboard / MSX++ official logo
                   \single_epbios_msx2plus_backslash     <=                 1chipMSX                with French    keyboard / MSX2+ logo
 1chipmsx_jp_layout\single_epbios_msxplusplus_yen        <=  this fw is for 1chipMSX                with Japanese  keyboard / MSX++ official logo
                   \single_epbios_msx2plus_yen           <=                 1chipMSX                with Japanese  keyboard / MSX2+ logo
 1chipmsx_us_layout\single_epbios_msxplusplus_backslash  <=  this fw is for 1chipMSX                with English   keyboard / MSX++ official logo   <=  default for 1chipMSX
                   \single_epbios_msx2plus_backslash     <=                 1chipMSX                with English   keyboard / MSX2+ logo

                                                                                                                                    { GROUP 2 }
      smx_br_layout\dual_epbios_smx_backslash            <=  this fw is for SM-X (regular)          with Brazilian keyboard /   Dual-EPBIOS
                   \single_epbios_smx_backslash          <=                 SM-X (regular)          with Brazilian keyboard / Single-EPBIOS
      smx_es_layout\dual_epbios_smx_backslash            <=  this fw is for SM-X (regular)          with Spanish   keyboard /   Dual-EPBIOS
                   \single_epbios_smx_backslash          <=                 SM-X (regular)          with Spanish   keyboard / Single-EPBIOS
      smx_fr_layout\dual_epbios_smx_backslash            <=  this fw is for SM-X (regular)          with French    keyboard /   Dual-EPBIOS
                   \single_epbios_smx_backslash          <=                 SM-X (regular)          with French    keyboard / Single-EPBIOS
      smx_it_layout\dual_epbios_smx_backslash            <=  this fw is for SM-X (regular)          with Italian   keyboard /   Dual-EPBIOS
                   \single_epbios_smx_backslash          <=                 SM-X (regular)          with Italian   keyboard / Single-EPBIOS
      smx_jp_layout\dual_epbios_smx_yen                  <=  this fw is for SM-X (regular)          with Japanese  keyboard /   Dual-EPBIOS
                   \single_epbios_smx_yen                <=                 SM-X (regular)          with Japanese  keyboard / Single-EPBIOS
      smx_us_layout\dual_epbios_smx_backslash            <=  this fw is for SM-X (regular)          with English   keyboard /   Dual-EPBIOS         <=  default for SM-X (regular)
                   \single_epbios_smx_backslash          <=                 SM-X (regular)          with English   keyboard / Single-EPBIOS

                                                                                                                                    { GROUP 3 }
  sx1mini_br_layout\single_epbios_sx1mini_backslash      <=  this fw is for SX-1 Mini/Mini+         with Brazilian keyboard
  sx1mini_es_layout\single_epbios_sx1mini_backslash      <=  this fw is for SX-1 Mini/Mini+         with Spanish   keyboard
  sx1mini_fr_layout\single_epbios_sx1mini_backslash      <=  this fw is for SX-1 Mini/Mini+         with French    keyboard
  sx1mini_jp_layout\single_epbios_sx1mini_yen            <=  this fw is for SX-1 Mini/Mini+         with Japanese  keyboard
  sx1mini_us_layout\single_epbios_sx1mini_backslash      <=  this fw is for SX-1 Mini/Mini+         with English   keyboard                         <=  default for SX-1 Mini/Mini+

                                                                                                                                    { GROUP 4 }
      sx2_br_layout\dual_epbios_sx2_backslash            <=  this fw is for SX-2                    with Brazilian keyboard /   Dual-EPBIOS
                   \single_epbios_sx2_backslash          <=                 SX-2                    with Brazilian keyboard / Single-EPBIOS
      sx2_es_layout\dual_epbios_sx2_backslash            <=  this fw is for SX-2                    with Spanish   keyboard /   Dual-EPBIOS
                   \single_epbios_sx2_backslash          <=                 SX-2                    with Spanish   keyboard / Single-EPBIOS
      sx2_fr_layout\dual_epbios_sx2_backslash            <=  this fw is for SX-2                    with French    keyboard /   Dual-EPBIOS
                   \single_epbios_sx2_backslash          <=                 SX-2                    with French    keyboard / Single-EPBIOS
      sx2_it_layout\dual_epbios_sx2_backslash            <=  this fw is for SX-2                    with Italian   keyboard /   Dual-EPBIOS
                   \single_epbios_sx2_backslash          <=                 SX-2                    with Italian   keyboard / Single-EPBIOS
      sx2_jp_layout\dual_epbios_sx2_yen                  <=  this fw is for SX-2                    with Japanese  keyboard /   Dual-EPBIOS
                   \single_epbios_sx2_yen                <=                 SX-2                    with Japanese  keyboard / Single-EPBIOS
      sx2_us_layout\dual_epbios_sx2_backslash            <=  this fw is for SX-2                    with English   keyboard /   Dual-EPBIOS         <=  default for SX-2
                   \single_epbios_sx2_backslash          <=                 SX-2                    with English   keyboard / Single-EPBIOS

                                                                                                                                    { GROUP 5 }
zemmixneo_br_layout\single_epbios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean       with Brazilian keyboard
                   \single_epbios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian    with Brazilian keyboard
                   \single_epbios_sx1_backslash          <=                 SX-1 (regular)          with Brazilian keyboard
zemmixneo_es_layout\single_epbios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean       with Spanish   keyboard
                   \single_epbios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian    with Spanish   keyboard
                   \single_epbios_sx1_backslash          <=                 SX-1 (regular)          with Spanish   keyboard
zemmixneo_fr_layout\single_epbios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean       with French    keyboard
                   \single_epbios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian    with French    keyboard
                   \single_epbios_sx1_backslash          <=                 SX-1 (regular)          with French    keyboard
zemmixneo_jp_layout\single_epbios_zemmixneo_yen          <=  this fw is for Zemmix Neo Korean       with Japanese  keyboard
                   \single_epbios_zemmixneobr_yen        <=                 Zemmix Neo Brazilian    with Japanese  keyboard
                   \single_epbios_sx1_yen                <=                 SX-1 (regular)          with Japanese  keyboard
zemmixneo_us_layout\single_epbios_zemmixneo_backslash    <=  this fw is for Zemmix Neo Korean       with English   keyboard                         <=  default for Zemmix Neo Korean
                   \single_epbios_zemmixneobr_backslash  <=                 Zemmix Neo Brazilian    with English   keyboard                         <=  default for Zemmix Neo Brazilian
                   \single_epbios_sx1_backslash          <=                 SX-1 (regular)          with English   keyboard                         <=  default for SX-1 (regular)


DIP-SW and Special Keys
=======================
GAMING-SPACEBAR     <=  [WIN]
GRAPH               <=  [F6] or [LALT]
KANA/CODE           <=  [F7] or [MENU]
SELECT              <=  [F8]
CTRL                <=  [LCTRL]
CANCEL              <=  [RALT]
EXECUTE             <=  [RCTRL]
CPU Clock           <=  [F12] or [DIP-SW1]
Video Output        <=  [(SHIFT+)PRTSCR] or [DIP-SW2/3]
Audio Mixer         <=  [(SHIFT+)PGUP/PGDOWN/F9/F10/F11]
Cartridge Slot-1    <=  [SHIFT+F12] or [DIP-SW4]
Cartridge Slot-2    <=  [SHIFT+SCRLK] or [DIP-SW5/6]
Internal Mapper     <=  [DIP-SW7] only
Internal MegaSD     <=  [DIP-SW8] only
Blackout Mode       <=  [PAUSE]
CMT                 <=  [SCRLK] on Cyclone I series     { 1chipMSX, Zemmix Neo (KR), Zemmix Neo BR, SX-1 (regular) and [SX-1 Mini/Mini+] }
Internal OPL3       <=  [SCRLK] on Cyclone IV-E series  { SM-X (regular) and SX-2 }
System Reset        <=  [HARD RESET KEY]  Three actions are possible:
                                          1. with a short click you can perform a quick reset;
                                          2. with a long click you can reload SDBIOS or EPBIOS;
                                          3. with one more click you can cancel the loading of SDBIOS to start EPBIOS instead.

Extra Keys on Cyclone IV-E series
=================================
Autofire ON/OFF     <=  [CTRL+SHIFT+PGUP] or [CTRL+SHIFT+PGDOWN]
Autofire Speed      <=  [CTRL+PGUP/PGDOWN]  Both LCTRL and RCTRL keys are available for Autofire functionality.
Autofire Status LED <=  [PAUSE]  The main LED blinks if Autofire is ON, otherwise it stays off in Blackout Mode.


______________
KdL 2022.09.24
