# mglOcm
rom file loader for 1chipMSX(KdL firmware machine)


### 'mglOcm' is a MSX ROM loader for the  "KdL firmware's OneChip MSX"

    that allows you to run msx rom cartridge images
    (like Konami-SCC, ASCII-8 and ASCII-16, 8, 16, 32k, linear rom files)
    on your device without setting any DIP switches or mapper patches.


Rom Loader for 1Chip MSX - 'mglOcm' v2.0370b (release date 2019/04/12)

v2.0370b :

## ABOUT

    - This is the loader application that support to execute megarom cartridge images
    like Konami-SCC, Ascii-8 and Ascii-16 all mappers for 1Chip-MSX(OCM).

    - 'mglOcm' is only for 1chip-MSX compatible loader which loads MSX-Rom image file
    needless to change any DIP switches and any mapper patches.

    - This is possible because 'mglOcm' use 1chipMSX's hardware mapper controller,
    if you using 'mglOcm' in load to rom image will complete supports ASCII8 and ASCII16 mappers
    and this executed megarom images perfectly.


### 1ChipMSX - Zemmix Neo
![1ChipMSX](ZemmixNeo.jpg)

### 1ChipMSX - IQ3000
![1ChipMSX](mglOcm.jpg)

### 1ChipMSX - SM-X
![1ChipMSX](SM-X.jpg)



## SPECIFICATIONS

        - Full MSX-DOS2, Nextor  support
        - Konami Mapper with SCC
        - ASCII 8 kB Mapper
        - ASCII 16 kB Mapper
        - Dualromimages load to OCM's internal memory slots.

## USAGE

        - MSXDOS2 must be loaded to run mglOcm.com

## Youtube Video Link
 - https://www.youtube.com/watch?v=oNPzevBzs64&list=PLlD0W14KLTkpq5dnONr_U6fAUWuyGliEw&index=80
 - https://www.youtube.com/watch?v=g5yTJ_7XwyQ&list=PLlD0W14KLTkpq5dnONr_U6fAUWuyGliEw&index=3


## Examples:

        - a:\roms> mglOcm gradius2.rom
        - a:\roms> mglOcm bublbobl.rom


## ...And more some command line options are as below.

        - /o = execute on Konami Classic Mapper
        - /s =    on Konami-SCC Mapper
        - /8 =    on Ascii-8 Mapper
        - /f =    on Ascii16 Mapper
        - /l =    on Linear  Mapper
        - /r = execute with alternative method
        - /t = Z80b 5.37MHz V9958 Fast mode
        - /k = Konami 2nd Cartridge secret option
        - /j = set Japanese keyboard layout
        - /d = back to DOS after loading

## REQUIREMENTS

        - MSX-DOS2, KdL firmware of v3.1 and over.

## CONTACT

- 'mglOcm' is written by ToughkidCST
- toughkiddev@gmail.com

