## The romdb.dat file contains information about rom mapper types

## Used by blueMSX. The format is one rom per line. The format of

## each line is:

## 

## [crc]  [romtype]  [description (optional)]

##

## All letters in the crc and rom type must be lower case.

##

## Rom types supported by the romdb are:

##

##        standard        Standard rom

##        msxdos2         MSX DOS 2 rom

##        konami5         Konami5 rom 

##        konami4         Konami4 rom

##        ascii8          ASCII8 rom

##        ascii16         ASCII16rom

##        ascii8sram      ASCII8 rom with SRAM

##        ascii16sram     ASCII16 rom with SRAM

##        koei            Koei rom with SRAM

##        gamemaster2     Game Master 2 rom

##        konami4nf       Konami4 variant (for cracked roms)

##        ascii16nf       ASCII16 variant (for cracked roms)

##        halnote         Halnote rom

##        basic           Basic rom (start at 0x8000)

##        0x4000          Standard rom (start at 0x4000)

##        fmpac           FM-PAC rom

##        rtype           R-TYPE rom

##        loderunner      Lode Runner rom

##        crossblaim      Crossblaim rom

##        harryfox        Harry Fox rom

##        korean80        Korean80 rom

##        korean126       Korean126 rom

##        holyquran       Holy Quran rom

##

                                           

CRC         ROM type          Description  

===         ========          ========     

cb935a50    basic             3d Golf      

27405eed    konami5           Space Manbow 

68fe9580    ascii16           Pinball Blaster