I imaged an MSX tape containing Spectravideo's `Swing Man` which is labelled as Spectravideo MSX release 221. The same software was written on both sides, though the copy on Side A had a single bit error not affecting functionality that was repaired by bandpassing. This software is a single tokenized BASIC file with tape file name `SM221` and is loaded using `CLOAD` and then started using `RUN`. The tokenized BASIC is identical to the version written inside the Aquarius cartridge version published in Thailand. This is a word-guessing game, and requires all letters to be entered in upper case. It exhibits graphical glitches on Japanese MSX'es due to the initially selected video mode.

CAS, BAS (tokenized BASIC) and ASC ("ASCII" BASIC) fingerprint information:
```
13K Swing Man (Side A) (Spectravideo) [_] [CLOAD-RUN].cas crc32:3d031bba md5:0804952e66b4560509f419440644ad2e sha1:d122e3c80cce689efe28dbb4734f411f6487ed98 sha256:8e0ebed82c4ec47e5f1869cbc2bc041eea9b67f47ea72d46a2f27f26d55eaac7 size:12570

13K Swing Man (Side B) (Spectravideo) [_] [CLOAD-RUN].cas crc32:3d031bba md5:0804952e66b4560509f419440644ad2e sha1:d122e3c80cce689efe28dbb4734f411f6487ed98 sha256:8e0ebed82c4ec47e5f1869cbc2bc041eea9b67f47ea72d46a2f27f26d55eaac7 size:12570

13K Swing Man (Spectravideo) [_] [CLOAD-RUN].cas crc32:3d031bba md5:0804952e66b4560509f419440644ad2e sha1:d122e3c80cce689efe28dbb4734f411f6487ed98 sha256:8e0ebed82c4ec47e5f1869cbc2bc041eea9b67f47ea72d46a2f27f26d55eaac7 size:12570

15K Swing Man (Spectravideo) [_].asc crc32:c1b5d998 md5:a10fc15c28d93d7459cd9f8534d91830 sha1:8071915372741d17d0e956205c3b5d08388bf445 sha256:869b55147e61ca2ccba464722f85a9bca3c7ca633ec692c5bda988f540eb345b size:15152

13K Swing Man (Spectravideo) [_].bas crc32:50934f96 md5:a08d472c354b3f25e9acd79595d4f806 sha1:2e1bc070850594085dac0bbab42bd80438760c96 sha256:8b92d32621a141f1021bf25491fc039eda758338290cea330601a77a46ef3e48 size:12539
```
Raw 24-bit stereo 44100 Hz FLAC audio was imaged using a Nakamichi BX-125 tape deck and a Steinberg UR22mkII USB ADC with Audacity under Win11 and is intended to be archival, CAS/ASC/BAS is for emulator use, and WAV is regenerated from CAS for the benefit of an actual MSX. Short filenames and long ones contain the same data.
